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We measured the roof of the skylights with a measuring tape at two locations, south and north (see map). Some roofs had two inverted terraces, breaking at the joints or contact of a lava, so we measured the uppermost roof and the thicker terrace behind. The lower measurement is perhaps not as accurate, because the height of the tape was estimated by eye from above (and below), but should be close.  

Door-entrance 
Height from top of crust to floor - 4.10 m 
Crustal measurements 
1.70 m (upper terrace), 2.40 m (lower terrace) 
Skylight 1 
West wall 3 flows, lower thickest 2.83 m 
Height from top of crust to floor at the northern end - 7.30 m 
Crustal measurements 
S1N 2.20 m (lower terrace), S1S 1.90 m
Skylight 2 
West wall, 5 flows, thickness about 1.4 m for the lowermost. 
Height from top of crust to floor at the northern end 9.80 m 
Crustal measurements 
S2N 90 cm, S2S 2.00 m 
Skylight 3 
West wall, 4 flows, the two in the middle have thicknesses 1.8 m (lower) and 2 m (upper). 
Height from top of crust to floor at the northern end 7.80 m
Crustal measurements 
S3N 2.20 m (upper terrace), 3.20 m (lower terrace), S3S 1.35 m (upper terrace), 2.50 m (lower terrace) 
Drillhole
The drillhole was located at the end of the touristic part of the cave close to the last lights, where the cave turns east. A yellow rope hangs out of the hole in the ceiling.  

